

# **Bellco Glass, Inc.**

*Equipment and Glassware Manufacturing*

*\*DISCLAIMER :The information contained in this specification sheet is correct to the best of our knowledge. The recommendations and suggestions therein are made without guarantee or representation as to the results. We recommend that adequate tests be made in your laboratory or plant to determine if this product meets all of your requirements.*

**Bellco Glass, Inc. services available for products and customers:**

* Technical Support
* Customer Service
* Application Support
* Hardware Support

**ABOUT OUR GLASS ITEMS**

Our manufacturing facility uses Type 1 Class A borosilicate glass. This is a type of glass that is of superior thermal and chemical resistance and specifically designed for volumetric glassware, providing you with products that give you longevity of use.

**TECHNICAL SUPPORT**

Technical support is available to all of our customers from inquiry to purchase and through the use of the product. Our service department is dedicated to ensuring the best white glove service to you as possible and to providing quality inspection and review of your concerns, should they arise.

**PRODUCT QUALITY**

Bellco Glass, Inc. guarantees quality in each and every product that goes out the door, from start to finish. With our strict QC policies and procedures, you can safely bet that you will get the best products Bellco Glass, Inc. has to offer with every single order.

**OUR VISION**

We will continue to move forward into the future with quality manufacturing, quality raw materials, and constantly redefining and upgrading our internal processes, thus, making us one of the best biotechnology manufacturing companies in the world.

*Bellco Glass, Inc. presents*

**Aseptic Sample System, 50mL**

SKU : 7909-00012



* For use with Bioreactor Vessels
* The sample system attaches to the head plate of a bioreactor, allowing the user to take repeated samples into a standard 50mL disposable centrifuge tube
* Samples are taken by evacuating air with supplied syringe and filter
* Assembly includes: Aseptic Sampler Cap (Cap, 2 Feed Tubes, and Extension Arm), Cap Gasket, 50cc Plastic Syringe, ¼” Female Quick Turn Barb, 0.2µm Filter (25mm OD), 50mL Polypropylene Centrifuge Tube, Silicone Connector Tube